3 bytes exchange between server-client

1. State available or not (255/0)
2. Notification(255/0)
3. Id
4. Server begins accepting sockets
5. Client connects to server
6. Server waits for data
7. Client sends info-network stream of 3 bytes
8. If state is available responds back to the client otherwise puts the state value to 0 again